Gemstone PhasorProtocols Library
Show/Hide TOC

# CommonFrameHeader Properties

## Properties

BinaryImage | Gets the binary image of the common header portion of this frame.
DataLength | Gets or sets the length of the data in the IEEE 1344 frame (i.e., the FrameLength minus the header length and checksum: FrameLength - 8).
FrameCount | Gets or sets the total frame count.
FrameImages | Gets or sets reference to a FrameImageCollector associated the IEEE 1344 frame, if any.
FrameLength | Gets or sets the entire length of the IEEE 1344 frame.
FrameType | Gets the fundamental frame type of this frame.
IsFirstFrame | Gets or sets flag from that determines if this is the first frame image in a series of images representing an entire frame.
IsLastFrame | Gets or sets flag that determines if this is the last frame image in a series of images representing an entire frame.
SampleCount | Gets or sets the sample number (i.e., frame count) of this frame.
State | Gets or sets the parsing state for the CommonFrameHeader object.
Timestamp | Gets or sets timestamp of this CommonFrameHeader.
TimeTag | Gets the timestamp of this frame in NTP format.
TypeID | Gets or sets the IEEE 1344 specific frame type of this frame.

## See Also

#### Reference

CommonFrameHeader Class
Gemstone.PhasorProtocols.IEEE1344 Namespace