Gemstone Numeric Library
Show/Hide TOC

# SignalKind Enumeration

Fundamental signal type enumeration for common EE measurements that represents a kind of signal, not an explicit type.

## Definition

Namespace: Gemstone.Numeric.EE
Assembly: Gemstone.Numeric (in Gemstone.Numeric.dll) Version: 1.0.163 -- Release Build+db050d8118fe22bfdd62897eda679bf877a0d036
C#
View Source Request Example

    [SerializableAttribute]
    public enum SignalKind

VB
View Source Request Example

    <SerializableAttribute>
    Public Enumeration SignalKind

C++
View Source Request Example

    [SerializableAttribute]
    public enum class SignalKind

JavaScript
View Source Request Example

    Gemstone.Numeric.EE.SignalKind = function();
    Gemstone.Numeric.EE.SignalKind.createEnum('Gemstone.Numeric.EE.SignalKind', false);

## Remarks

This enumeration represents the basic type of a signal used to suffix a formatted signal reference. When used in context along with an optional index the fundamental signal type will identify a signal's location within a frame of data (see SignalReference).

Contrast this to the SignalType enumeration which further defines an explicit type for a signal (e.g., a voltage or current type for an angle).

## Members

Angle | 0 | Phase angle.
Magnitude | 1 | Phase magnitude.
Frequency | 2 | Line frequency.
DfDt | 3 | Frequency delta over time (dF/dt).
Status | 4 | Status flags.
Digital | 5 | Digital value.
Analog | 6 | Analog value.
Calculation | 7 | Calculated value.
Statistic | 8 | Statistical value.
Alarm | 9 | Alarm value.
Quality | 10 | Quality flags.
PoWCurrent | 11 | Point-on-wave current.
PoWVoltage | 12 | Point-on-wave voltage.
Unknown | 13 | Undetermined signal type.

## See Also

#### Reference

Gemstone.Numeric.EE Namespace