Gemstone PhasorProtocols Library
Show/Hide TOC

# FrameParser Events

## Events

BufferParsed | Occurs when buffer parsing has completed. (Inherited from BinaryImageParserBase)
ConfigurationChanged | Occurs when a device sends a notification that its configuration has changed. (Inherited from FrameParserBaseTFrameIdentifier)
DataDiscarded | Occurs when data image fails deserialized due to an exception. (Inherited from BinaryImageParserBase)
DataParsed | Occurs when a data image is deserialized successfully to one of the output types that the data image represents. (Inherited from FrameImageParserBase FrameType, ISupportSourceIdentifiableFrameImage SourceChannel, FrameType)
DuplicateTypeHandlerEncountered | Occurs when more than one type has been defined that can deserialize the specified output type. (Inherited from FrameImageParserBase FrameType, ISupportSourceIdentifiableFrameImage SourceChannel, FrameType)
OutputTypeNotFound | Occurs when matching an output type for deserializing the data image could not be found. (Inherited from FrameImageParserBase FrameType, ISupportSourceIdentifiableFrameImage SourceChannel, FrameType)
ParsingException | Occurs when an Exception is encountered while attempting to parse data. (Inherited from BinaryImageParserBase)
ReceivedChannelFrame | Occurs when any IChannelFrame has been received. (Inherited from FrameParserBaseTFrameIdentifier)
ReceivedCommandFrame | Occurs when a ICommandFrame has been received. (Inherited from FrameParserBaseTFrameIdentifier)
ReceivedConfigurationFrame | Occurs when a SEL CWS ConfigurationFrame has been received.
ReceivedDataFrame | Occurs when a SEL CWS DataFrame has been received.
ReceivedFrameBufferImage | Occurs when a frame image has been received, event includes buffer. (Inherited from FrameParserBaseTFrameIdentifier)
ReceivedFrameImage | Occurs when a frame image has been received. (Inherited from FrameParserBaseTFrameIdentifier)
ReceivedHeaderFrame | Occurs when a IHeaderFrame has been received. (Inherited from FrameParserBaseTFrameIdentifier)
ReceivedUndeterminedFrame | Occurs when an undetermined IChannelFrame has been received. (Inherited from FrameParserBaseTFrameIdentifier)
SourceDataParsed | Occurs when a data image is deserialized successfully to one or more of the output types that the data image represents. (Inherited from MultiSourceFrameImageParserBase SourceChannel, FrameType, ISupportSourceIdentifiableFrameImage SourceChannel, FrameType)

## See Also

#### Reference

FrameParser Class
Gemstone.PhasorProtocols.SelCWS Namespace